# This file contains lines that are used.
# Comments about rules that should be implemented are retained.
# Specifications in Data.C of type are not in this file

# Standard Outputs and Input Specifications for watch window
#
## Blocks that are added as standard use these forms of statements:
##
## FCx block N included in watch window
## FCx block N+12 included in watch window
## FCx block N through N+1 included in watch window
## FCx block N+1 through N+32 included in watch window
## FCx S1 included in watch window 
## FCx S1 through S2 included in watch window
## FCx S10 through S11 included in watch window 
##
## Multiple statements per FC type will work, allowing gaps in the selected blocks
##
## The following statement flags FC types that have no standard outputs or inputs
##
## FCx not included in watch window

# FC1 FUNCTION GENERATOR
FC1 block N included in watch window
FC1 S1 included in watch window 

# FC2 MANUAL SET CONSTANT
FC2 not included in watch window

# FC3 LEAD/LAG
FC3 block N included in watch window
FC3 S1 included in watch window 

# FC4 PULSE/POSITIONER
FC4 block N through N+1 included in watch window
FC4 S1 through S2 included in watch window 

# FC5 PULSE RATE
FC5 block N included in watch window
FC5 S1 included in watch window 

# FC6 HIGH/LOW LIMITER
FC6 block N included in watch window
FC6 S1 included in watch window 

# FC7 SQUARE ROOT
FC7 block N included in watch window
FC7 S1 included in watch window 

# FC8 RATE LIMIT
FC8 block N included in watch window
FC8 S1 included in watch window 

# FC9 TRANSFER - ANALOG
FC9 block N included in watch window
FC9 S1 through S2 included in watch window 

# FC10 HIGH SELECT
FC10 block N included in watch window
FC10 S1 through S4 included in watch window 

# FC11 LOW SELECT
FC11 block N included in watch window
FC11 S1 through S4 included in watch window 

# FC12 HIGH/LOW ALARM
FC12 block N has state 1 HIGH
FC12 block N+1 has state 1 LO
FC12 block N through N+1 included in watch window
FC12 S1 included in watch window

# FC13 INTEGER TRANSFER
FC13 block N included in watch window
FC13 S1 through S2 included in watch window 

# FC14 SUM 4-INPUT
FC14 block N included in watch window
FC14 S1 through S4 included in watch window 

# FC15 SUM 2-INPUT
FC15 block N included in watch window
FC15 S1 through S2 included in watch window 

# FC16 MULTIPLY
FC16 block N included in watch window
FC16 S1 through S2 included in watch window 

# FC17 DIVIDE
FC17 block N included in watch window
FC17 S1 through S2 included in watch window 

# FC18 PID CONTROLLER/ERROR IN
FC18 block N included in watch window
FC18 S1 included in watch window 

# FC19 PID CONTROL/PV & SP INPUTS
FC19 block N included in watch window
FC19 S1 through S2 included in watch window 

# FC20 INDICATOR STATION
FC20 S1 through S3 included in watch window 

# FC21 BASIC STATION MAN/AUTO TRANSFER STATION
FC21 block N+2 has state 0 MANL
FC21 block N+2 has state 1 AUTO
FC21 block N+3 has state 0 LOCAL
FC21 block N+3 has state 1 CMPUTR
FC21 block N+5 has state 1 TIMOUT
FC21 block N through N+1 included in watch window
FC21 S1 included in watch window

# FC22 CASC STATION MAN/AUTO TRANSFER STATION
FC22 block N+2 has state 0 MANL
FC22 block N+2 has state 1 AUTO
FC22 block N+3 has state 0 LOCAL
FC22 block N+3 has state 1 CMPUTR
FC22 block N+4 has state 0 BASIC
FC22 block N+4 has state 1 CASC
FC22 block N+5 has state 1 TIMOUT
FC22 block N through N+1 included in watch window
FC22 S1 included in watch window

# FC23 RATIO STATION M/A TRANSFER STATION
FC23 block N+2 has state 0 MANL
FC23 block N+2 has state 1 AUTO
FC23 block N+3 has state 0 LOCAL
FC23 block N+3 has state 1 CMPUTR
FC23 block N+4 has state 0 BASIC
FC23 block N+4 has state 1 RATIO
FC23 block N+5 has state 1 TIMOUT
FC23 block N through N+1 included in watch window
FC23 S1 included in watch window

# FC24 ADAPT
FC24 S1 included in watch window

# FC25 ANALOG INPUT (SAME PCU)
FC25 block N has quality
FC25 block N imports quality
FC25 block N included in watch window

# FC26 ANALOG INPUT (DIFFERENT PCU)
FC26 block N has quality
FC26 block N imports quality
FC26 block N included in watch window

# FC27 ANALOG INPUT(TERMINATION UNIT - TCS)
FC27 block N has quality
FC27 block N included in watch window

# FC28 ANALOG OUTPUT(SAME PCU)
FC28 block N has quality
FC28 block N has communications quality
FC28 block N included in watch window

# FC29 ANALOG OUTPUT(TERMINATION UNIT - TCS)
FC29 block N has quality
FC29 block N has communications quality
FC29 block N included in watch window

# FC30 ANALOG EXCEPTION REPORT
FC30 block N has quality
FC30 block N propagates quality from S1
FC30 block N included in watch window

# FC31 TEST QUALITY
FC31 S1,S2,S3,S4 must be wired from quality
FC31 block N included in watch window
FC31 S1 through S4 included in watch window 

# FC32 TRIP
FC32 block N has state 0 NORMAL
FC32 block N has state 1 TRIPPD
FC32 not included in watch window

# FC33 NOT
FC33 block N included in watch window

# FC34 MEMORY
FC34 block N included in watch window
FC34 S1 through S2 included in watch window 

# FC35 TIME DELAY OR PULSE
FC35 block N included in watch window
FC35 S1 included in watch window 

# FC36 QUALIFIED OR 8-INPUT
FC36 block N included in watch window
FC36 S1 through S8 included in watch window 

# FC37 AND 2-INPUT
FC37 block N included in watch window
FC37 S1 through S2 included in watch window 

# FC38 AND 4-INPUT
FC38 block N included in watch window
FC38 S1 through S4 included in watch window 

# FC39 OR 2-INPUT
FC39 block N included in watch window
FC39 S1 through S2 included in watch window 

# FC40 OR 4-INPUT
FC40 block N included in watch window
FC40 S1 through S4 included in watch window 

# FC41 DIGITAL INPUT (SAME PCU)
FC41 block N has quality
FC41 block N imports quality
FC41 block N included in watch window

# FC42 DIGITAL INPUT (DIFFERENT PCU)
FC42 block N has quality
FC42 block N imports quality
FC42 block N included in watch window

# FC43 DIGITAL INPUT/TCS
FC43 block N has quality
FC43 block N included in watch window

# FC44 DIGITAL OUTPUT/TCS
FC44 block N has quality
FC44 block N has communications quality
FC44 block N included in watch window

# FC45 DIGITAL EXCEPTION REPORT
FC45 block N has quality
FC45 block N propagates quality from S1
FC45 block N included in watch window

# FC46 DIGITAL INPUT LIST(SAME PCU)
FC46 block N-N+7 has quality
FC46 block N-N+7 has communications quality
FC46 block N through N+7 included in watch window

# FC47 ANALOG INPUT (TERMINATION UNIT-TAI)
FC47 not included in watch window

# FC48 ANALOG EXCEPTION REPORT WITH DEADBAND
FC48 block N has quality
FC48 block N propagates quality from S1
FC48 block N included in watch window

# FC49 DIGITAL OUTPUT BUFFER
FC49 block N included in watch window

# FC50 MANUAL SET SWITCH
FC50 block N included in watch window

# FC51 MANUAL SET CONSTANT
FC51 block N included in watch window

# FC52 MANUAL SET INTEGER
FC52 block N included in watch window

# FC53 EXECUTIVE CONTROLLER MODULE
FC53 not included in watch window

# FC54 EXECUTIVE LOGIC MASTER MODULE
FC54 not included in watch window

# FC55 HYDRAULIC SERVO SLAVE
FC55 block N-N+5 has quality
FC55 block N+8 has state 0 GOOD
FC55 block N+8 has state 1 BAD
FC55 block N+9 has state 0 GOOD
FC55 block N+9 has state 1 BAD
FC55 block N through N+5 included in watch window

# FC56 EXEC ANALOG MASTER MODULE (HI LEVEL)
FC56 not included in watch window

# FC57 NODE STATISTICS BLOCK
FC57 not included in watch window

# FC58 ANALOG TIME DELAY
FC58 block N included in watch window
FC58 S1 through S2 included in watch window 

# FC59 TRANSFER DIGITAL
FC59 block N included in watch window
FC59 S1 through S2 included in watch window 

# FC60 GROUP I/O DEFINITION BLOCK
FC60 not included in watch window

# FC61 BLINK
FC61 block N included in watch window
FC61 S1 through S2 included in watch window 

# FC62 REMOTE CONTROL MEMORY
FC62 block N included in watch window
FC62 S1 through S7 included in watch window 

# FC63 ANALOG INPUT LIST (8)(SAME PCU)
FC63 block N-N+7 has quality
FC63 block N-N+7 imports quality
FC63 block N through N+7 included in watch window

# FC64 DIGITAL INPUT LIST (8)(SAME PCU)
FC64 block N-N+7 has quality
FC64 block N-N+7 imports quality
FC64 block N through N+7 included in watch window

# FC65 4 - INPUT DIGITAL SUM WITH GAIN
FC65 block N included in watch window
FC65 S1 through S4 included in watch window 

# FC66 ANALOG TREND
FC66 block N included in watch window
FC66 S1 included in watch window 

# FC67 DIGITAL EXCEPTION REPORT WITH DEADBAND
FC67 block N has quality
FC67 block N propagates quality from S1
FC67 block N included in watch window

# FC68 REMOTE MANUAL SET CONSTANT
FC68 block N included in watch window

# FC69 TEST ALARM
FC69 block N through N+1 included in watch window

# FC70 ANALOG INPUT - EXCEPT REP AND ALARM
FC70 block N included in watch window

# FC71 EXEC - ANALOG MASTER MOD (AMM02)
FC71 not included in watch window

# FC72 SLAVE DEFINITION BLOCK
FC72 not included in watch window

# FC73 CALIBRATION DATA BLOCK
FC73 block N included in watch window

# FC74 CALIBRATION COMMAND BLOCK
FC74 not included in watch window

# FC75 CALIBRATION STATUS BLOCK
FC75 not included in watch window

# FC76 THERMOCOUPLE TU TEMPERATURE BLOCK
FC76 block N through N+3 included in watch window

# FC77 ANALOG POINT SERVICE STATUS
FC77 not included in watch window

# FC78 TREND DEFINITION BLOCK
FC78 not included in watch window

# FC79 CIS INTERFACE BLOCK
FC79 block N through N+8 has quality
FC79 block N+9 has state 0 GOOD
FC79 block N+9 has state 1 BAD
FC79 block N through N+5 included in watch window
FC79 S10 through S11 included in watch window
FC79 S15 through S18 included in watch window

# FC80 CONTROL STATION (MFP/MFC)
FC80 block N+2 has state 0 MAN
FC80 block N+2 has state 1 AUT
FC80 block N+3 has state 0 LOCAL
FC80 block N+3 has state 1 CMPUTR
FC80 block N+4 has state 0 BAS
FC80 block N+4 has state 1 C/R
FC80 block N through N+1 always included in watch window
FC80 S1 included in watch window
# FC80 block N+5 must not show FAILED, as it is no longer used in modern consoles

# FC81 EXECUTIVE (MFP/MFC)
FC81 block N has state 1 STRTUP
FC81 block N+2 included in watch window

# FC82 SEGMENT CONTROL (MFP/MFC)
FC82 block N through N+4 included in watch window

# FC83 DIGITAL OUTPUT GROUP
FC83 block N has state 0 GOOD
FC83 block N has state 1 BAD
FC83 S4 through S11 included in watch window 

# FC84 DIGITAL INPUT GROUP
FC84 block N through N+7 has quality
FC84 block N through N+7 included in watch window

# FC85 UP/DOWN COUNTER
FC85 block N+1 has state 1 HIGH
FC85 block N+2 has state 1 LOW
FC85 block N included in watch window
FC85 S1 through S2 included in watch window 

# FC86 ELAPSED TIMER
FC86 block N+1 has state 1 ELAPSD
FC86 block N included in watch window

# FC87 LOGIC STATION INTERFACE
FC87 block N has state 0 GOOD
FC87 block N has state 1 BAD
FC87 not included in watch window

# FC88 LOGIC STATION
FC88 block N has state 0 OPEN
FC88 block N has state 1 CLOSED
FC88 block N+1 has state 0 OPEN
FC88 block N+1 has state 1 CLOSED
FC88 block N+2 has state 0 OPEN
FC88 block N+2 has state 1 CLOSED
FC88 block N+3 has state 0 OPEN
FC88 block N+3 has state 1 CLOSED
FC88 block N+4 has state 0 OPEN
FC88 block N+4 has state 1 CLOSED
FC88 block N+5 has state 0 OPEN
FC88 block N+5 has state 1 CLOSED
FC88 block N+6 has state 0 OPEN
FC88 block N+6 has state 1 CLOSED
FC88 block N+7 has state 0 OPEN
FC88 block N+7 has state 1 CLOSED
FC88 block N+8 has state 0 GOOD
FC88 block N+8 has state 1 BAD
FC88 not included in watch window

# FC89 HIGH BLOCK LIMIT
FC89 not included in watch window

# FC90 EXTENDED EXECUTIVE (MFP/MFC)
FC90 block N+3 has state 0 INVALD
FC90 not included in watch window

# FC91 BASIC CONFIGURATION BLOCK
FC91 block N included in watch window

# FC92 BASIC EXECUTION BLOCK
FC92 block N included in watch window

# FC93 BASIC OUTPUT BUFFER - REAL
FC93 block N through N+3 included in watch window

# FC94 BASIC OUTPUT BUFFER - BOOLEAN
FC94 block N through N+3 included in watch window

# FC95 MODULE STATUS MONITOR
FC95 block N has quality
FC95 block N has state 0 GOOD
FC95 block N has state 1 BAD
FC95 not included in watch window

# FC96 REDUNDANT ANALOG INPUT
FC96 block N has quality
FC96 block N included in watch window
FC96 S1 through S2 included in watch window 

# FC97 REDUNDANT DIGITAL INPUT
FC97 block N has quality
FC97 block N included in watch window
FC97 S1 through S2 included in watch window 

# FC98 REDUNDANT SLAVE SELECT
FC98 S3 S4 S7 S8 must be wired from quality
FC98 block N has state 0 MOD_1
FC98 block N has state 1 MOD_2
FC98 block N+1 has state 0 GOOD
FC98 block N+1 has state 1 BAD
FC98 block N through N+1 included in watch window
FC98 S1 through S9 included in watch window 

# FC99 SEQUENCE-OF-EVENTS LOG
FC99 block N has state 1 LOGGED
FC99 not included in watch window

# FC100 DIGITAL OUTPUT READBACK CHECK
FC100 block N has state 0 OK
FC100 block N has state 1 FAULT
FC100 block N included in watch window
FC100 S1 through S16 included in watch window 

# FC101 XOR - INPUT
FC101 block N included in watch window
FC101 S1 through S2 included in watch window 

# FC102 PULSE INPUT/PERIOD
FC102 block N+1 has state 1 HIGH
FC102 block N+2 has state 1 LOW
FC102 block N+3 has state 0 GOOD
FC102 block N+3 has state 1 BAD
FC102 block N has quality
FC102 block N included in watch window

# FC103 PULSE INPUT/FREQUENCY COUNTER
FC103 block N+1 has state 1 HIGH
FC103 block N+2 has state 1 LOW
FC103 block N+3 has state 0 GOOD
FC103 block N+3 has state 1 BAD
FC103 block N has quality
FC103 block N included in watch window

# FC104 PULSE INPUT/TOTALIZATION
FC104 block N+1 has state 1 ALARM
FC104 block N+2 has state 0 GOOD
FC104 block N+2 has state 1 BAD
FC104 block N has quality
FC104 block N included in watch window

# FC105 EXECUTIVE BLOCK (LMM02)
FC105 not included in watch window

# FC106 SEGMENT CONTROL BLOCK (LMM02)
FC106 block N through N+2 included in watch window

# FC107 GROUP I/O DEFINITION (LMM02)
FC107 block N has state 0 GOOD
FC107 block N has state 1 BAD
FC107 not included in watch window

# FC108 EXTENDED EXECUTIVE - LMM02
FC108 block N through N+1 included in watch window

# FC109 PULSE INPUT/DURATION
FC109 block N+1 has state 1 HIGH
FC109 block N+2 has state 1 LOW
FC109 block N+3 has state 0 GOOD
FC109 block N+3 has state 1 BAD
FC109 block N has quality
FC109 block N included in watch window

# FC110 5 INPUT RUNG
FC110 block N included in watch window
FC110 S7 through S11 included in watch window

# FC111 10 INPUT RUNG
FC111 block N included in watch window
FC111 S12 through S21 included in watch window

# FC112 20 INPUT RUNG
FC112 block N included in watch window
FC112 S22 through S41 included in watch window

# FC113 ASCII STRING DESCRIPTOR
FC113 not included in watch window

# FC114 P.L.C. BCD INPUT
FC114 block N has quality 
FC114 block N included in watch window

# FC115 P.L.C. BCD OUTPUT
FC115 block N has state 0 GOOD
FC115 block N has state 1 BAD
FC115 S4 included in watch window

# FC116 JUMP/MASTER CONTROL RELAY
FC116 block N has state 0 JUMP
FC116 not included in watch window

# FC117 BOOLEAN RECIPE TABLE
FC117 block N included in watch window

# FC118 REAL RECIPE TABLE
FC118 block N included in watch window

# FC119 BOOLEAN SIGNAL MUX
FC119 block N included in watch window
FC119 S1 through S11 included in watch window

# FC120 REAL SIGNAL MUX
FC120 block N included in watch window
FC120 S1 through S11 included in watch window

# FC121 ANALOG INPUT/SUPERLOOP
FC121 block N has quality 
FC121 block N imports quality
FC121 block N included in watch window

# FC122 DIGITAL INPUT/SUPERLOOP
FC122 block N has quality
FC122 block N imports quality 
FC122 block N included in watch window

# FC123 DEVICE DRIVER
FC123 block N included in watch window
FC123 S1 through S3 included in watch window

# FC124 SEQUENCE MONITOR
FC124 block N through N+1 included in watch window
FC124

# FC125 DEVICE MONITOR
FC125 block N included in watch window
FC125 S1 through S16 included in watch window

# FC126 REAL SIGNAL DEMULTIPLEXER
FC126 block N through N+7 included in watch window
FC126 S1 through S12 included in watch window 

# FC127 PLANT LOOP GATEWAY NODE MAP
FC127 not included in watch window

# FC128 SLAVE DEFAULT DEFINITION
FC128 not included in watch window

# FC129 MULTI-STATE DEVICE DRIVER
FC129 block N through N+3 included in watch window
FC129 S1 through S6 included in watch window
FC129 S25 included in watch window

# FC130 PLANT LOOP GATEWAY EXECUTIVE
FC130 block N-N+1 has quality
FC130 block N-N+1 has communication quality
FC130 not included in watch window

# FC131 PLANT LOOP GATEWAY POINT DEFINITION
FC131 block N has quality
FC131 block N has communication quality
FC131 not included in watch window

# FC132 ANALOG INPUT/SLAVE
FC132 block N-N+4 has quality
FC132 block N+5 has state 0 GOOD
FC132 block N+5 has state 1 BAD
FC132 block N through N+4 included in watch window

# FC133 SMART TRANSMITTER DEFINITION
FC133 block N has state 0 GOOD
FC133 block N has state 1 BAD
FC133 S1 included in watch window 

# FC134 MULTI SEQUENCE MONITOR
FC134 block N+4 has state 0 INSERT
FC134 block N+4 has state 1 DONE
FC134 block N+5 has state 0 RUN
FC134 block N+5 has state 1 HOLD
FC134 block N through N+5 included in watch window

# FC135 SEQUENCE MANAGER
FC135 block N has state 0 RESET
FC135 block N has state 1 HOLD
FC135 block N through N+2 included in watch window

# FC136 REMOTE MOTOR CONTROL
FC136 block N has state 0 STOP
FC136 block N has state 1 RUN
FC136 block N included in watch window
FC136 S1 through S10 included in watch window 

# FC137 BASIC REAL OUTPUT BUFFER WITH QUALITY
FC137 block N through N+3 has quality
FC137 block N through N+3 included in watch window

# FC138 BASIC BOOLEAN OUTPUT BUFFER WITH QUALITY
FC138 block N through N+3 has quality
FC138 block N through N+3 included in watch window

# FC139 PASSIVE STATION INTERFACE
FC139 block N has state 1 AUTBYP
FC139 not included in watch window

# FC140 RESTORE
FC140 not included in watch window

# FC141 SEQUENCE MASTER
FC141 block N through N+4 included in watch window

# FC142 SEQUENCE SLAVE
FC142 not included in watch window

# FC143 INVOKE C
FC143 block N included in watch window

# FC144 C ALLOCATION
FC144 not included in watch window

# FC145 FREQUENCY COUNTER SLAVE INTERFACE
FC145 block N has quality
FC145 block N+1 has state 1 HIGH
FC145 block N+2 has state 1 LOW
FC145 block N+3 has state 0 GOOD
FC145 block N+3 has state 1 BAD
FC145 block N included in watch window

# FC146 REMOTE I/O INTERFACE
FC146 block N has state 0 GOOD
FC146 block N has state 1 BAD
FC146 block N+1 has state 0 GOOD
FC146 block N+1 has state 1 BAD
FC146 block N+2 included in watch window

# FC147 REMOTE I/O DEFINITION
FC147 block N has state 0 GOOD
FC147 block N has state 1 BAD
FC147 not included in watch window

# FC148 BATCH SEQUENCE
FC148 block N+2 has state 0 HOLD
FC148 block N+2 has state 1 RUN
FC148 block N+3 has state 0 NOTFLT
FC148 block N+3 has state 1 FAULT
FC148 block N+4 has state 0 NOTHLD
FC148 block N+4 has state 1 HOLD
FC148 block N+5 has state 0 INCOMP
FC148 block N+5 has state 1 COMPLT
FC148 block N+6 has state 0 NOTRST
FC148 block N+6 has state 1 RESET
FC148 block N through N+1 included in watch window

# FC149 ANALOG OUTPUT/SLAVE
FC149 block N-N+6 has quality
FC149 block N through N+6 included in watch window
FC149 S4 through S10 included in watch window

# FC150 HYDRAULIC SERVO SLAVE INTERFACE
FC150 block N has quality
FC150 block N+1 has state 0 NOTNUL
FC150 block N+1 has state 1 NULL
FC150 block N+2 has state 0 GOOD
FC150 block N+2 has state 1 BAD
FC150 block N+3 has state 0 GOOD
FC150 block N+3 has state 1 BAD
FC150 block N+4 has state 0 GOOD
FC150 block N+4 has state 1 BAD
FC150 block N+5 has state 0 GOOD
FC150 block N+5 has state 1 BAD
FC150 block N+6 has state 0 GOOD
FC150 block N+6 has state 1 BAD
FC150 block N+7 has state 0 GOOD
FC150 block N+7 has state 1 BAD
FC150 block N included in watch window

# FC151 TEXT SELECTOR
FC151 block N included in watch window

# FC152 PARAMETER ESTIMATOR
FC152 block N+4 has state 0 LOCKED
FC152 block N+4 has state 1 ESTIM
FC152 block N through N+3 included in watch window
FC152 S1 through S2 included in watch window

# FC153 PARAMETER CONVERTER
FC153 block N through N+3 included in watch window
FC153 S1 through S4 included in watch window

# FC154 ADAPTIVE PARAMETER SCHEDULER
FC154 block N through N+2 included in watch window
FC154 S1 through S3 included in watch window

# FC155 REGRESSION
FC155 block N+9 has state 0 COMPUT
FC155 block N+9 has state 1 DFAULT
FC155 block N through N+8 included in watch window
FC155 S1 through S5 included in watch window

# FC156 ADVANCED PID
FC156 block N+1 has state 0 PERMIT
FC156 block N+1 has state 1 INHIBT
FC156 block N+2 has state 0 PERMIT
FC156 block N+2 has state 1 INHIBT
FC156 block N included in watch window
FC156 S1 through S2 included in watch window
FC156 S6 included in watch window

# FC157 GENERAL DIGITAL CONTROLLER
FC157 block N included in watch window
FC157 S1 through S2 included in watch window
FC157 S4 included in watch window

# FC158 ENHANCED ANALOG PT. DEFIN
FC158 block N has quality
FC158 block N included in watch window

# FC159 POLYNOMIAL ADJUSTMENT
FC159 not included in watch window

# FC160 SMITH PREDICTOR
FC160 block N included in watch window
FC160 S1 through S2 included in watch window
FC160 S5 included in watch window

# FC161 SEQUENCE GENERATOR
FC161 block N through N+9 included in watch window

# FC162 SEGMENT BUFFER/DIGITAL
FC162 block N through N+3 included in watch window

# FC163 SEGMENT BUFFER/ANALOG
FC163 block N through N+3 included in watch window

# FC164 SEGMENT CONTROL BLOCK
FC164 block N through N+1 included in watch window

# FC165 MOVING AVERAGE
FC165 block N included in watch window
FC165 S1 included in watch window

# FC166 INTEGRATOR
FC166 block N+1 has state 0 GOOD
FC166 block N+1 has state 1 LIMIT
FC166 block N included in watch window
FC166 S1 included in watch window

# FC167 POLYNOMIAL (SEVENTH ORDER)
FC167 block N included in watch window
FC167 S1 included in watch window

# FC168 INTERPOLATOR
FC168 block N+1 has state 0 GOOD
FC168 block N+1 has state 1 LIMIT
FC168 block N included in watch window
FC168 S1 through S2 included in watch window

# FC169 MATRIX ADD (3 X 3)
FC169 block N through N+8 included in watch window
FC169 S1 through S18 included in watch window

# FC170 MATRIX MULTIPLY (3 X 3)
FC170 block N through N+8 included in watch window
FC170 S1 through S18 included in watch window

# FC171 TRIG
FC171 block N included in watch window
FC171 S1 included in watch window

# FC172 EXPONENTIAL
FC172 block N included in watch window
FC172 S1 included in watch window

# FC173 POWER
FC173 block N included in watch window
FC173 S1 through S2 included in watch window

# FC174 LOGARITHM
FC174 block N included in watch window
FC174 S1 included in watch window

# FC175 EXECUTIVE (CSC)
FC175 block N+12 included in watch window

# FC176 SEQUENCE STATION
FC176 not included in watch window

# FC177 DATA ACQUISITION ANALOG
FC177 block N has quality
FC177 block N included in watch window
FC177 S10 included in watch window

# FC178 DATA ACQUISITION ANALOG INPUT/LOOP
FC178 block N has quality
FC178 block N has communication quality
FC178 block N has process quality
FC178 block N included in watch window

# FC179 ENHANCED TREND DEFINITION
FC179 block N has quality
FC179 block N+1 included in watch window

# FC180 BATCH INPUT/OUTPUT
FC180 block N through N+11 included in watch window

# FC181 BATCH STATION (CBC)
FC181 

# FC182 ANALOG INPUT DEFINITION
FC182 block N has quality
FC182 block N included in watch window

# FC183 BATCH EXECUTIVE (CBC)
FC183 block N+12 included in watch window

# FC184 FIP SLAVE HANDLER
FC184 block N has state 0 GOOD
FC184 block N has state 1 BAD
FC184 block N+1 has state 0 GOOD
FC184 block N+1 has state 1 BAD
FC184 not included in watch window

# FC185 DIGITAL INPUT SUBSCRIBER
FC185 block N through N+7 has quality
FC185 block N through N+7 included in watch window

# FC186 ANALOG INPUT SUBSCRIBER
FC186 block N through N+7 has quality
FC186 block N through N+7 included in watch window

# FC187 ANALOG OUTPUT SUBSCRIBER
FC187 S4 through S11 included in watch window

# FC188 DIGITAL OUTPUT SUBSCRIBER
FC188 S4 through S11 included in watch window

# FC189 Not Implemented
FC189 not included in watch window

# FC190 UDF DECLARATION
FC190 not included in watch window

# FC191 UDF1
FC191 block N through N+1 included in watch window
FC191 block N through N+1 has quality

# FC192 UDF2
FC192 block N through N+9 included in watch window
FC192 S1 through S18 included in watch window
FC192 block N through N+9 has quality

# FC193 USER DEFINED DATA IMPORT BLOCK
FC193 block N has quality
FC193 block N included in watch window

# FC194 USER DEFINED DATA EXPORT BLOCK
FC194 block N has quality
FC194 not included in watch window

# FC195 Not Implemented
FC195 not included in watch window

# FC196 Not Implemented
FC196 not included in watch window

# FC197 Not Implemented
FC197 not included in watch window

# FC198 AUXILIARY REAL UDF
FC198 block N through N+3 included in watch window
FC198 S1 through S4 included in watch window
FC198 block N through N+3 has quality

# FC199 AUXILIARY DIGITAL UDF
FC199 block N through N+3 included in watch window
FC199 S1 through S4 included in watch window
FC199 block N through N+3 has quality

# FC200 LOCAL INFINET/PLANTLOOP GATEWAY EXECUTIV
FC200 not included in watch window

# FC201 INFINET DATA POINT DEFINITION
FC201 not included in watch window

# FC202 INFINET-TO-INFINET TRANSFER MODULE EXEC
FC202 not included in watch window

# FC203 INFI-NET TO PLANT LOOP TRANSFER EXEC BLK
FC203 not included in watch window

# FC204 Not Implemented
FC204 not included in watch window

# FC205 ANALOG INPUT LIST/CW800
FC205 block N-N+7 has quality
FC205 block N-N+7 has communications quality
FC205 block N through N+7 included in watch window

# FC206 DIGITAL INPUT LIST/CW800
FC206 block N-N+7 has quality
FC206 block N-N+7 has communications quality
FC206 block N through N+7 included in watch window

# FC207 MODULE STATUS MONITOR/CW800
FC207 block N has quality
FC207 block N has communications quality
FC207 not included in watch window

# FC208 Not Implemented
FC208 not included in watch window

# FC209 Not Implemented
FC209 not included in watch window

# FC210 SEQUENCE-OF-EVENTS SLAVE
FC210 block N+1-N+32 has quality
FC210 block N has state 0 NO_LOG
FC210 block N has state 1 LOGGED
FC210 block N+1 through N+32 included in watch window

# FC211 DATA ACQUISITION DIGITAL
FC211 block N has quality
FC211 block N included in watch window

# FC212 DATA ACQUISITION DIGITAL INPUT/LOOP
FC212 block N has quality
FC212 block N has communication quality
FC212 block N has process quality
FC212 block N included in watch window

# FC213 Not Implemented
FC213 not included in watch window

# FC214 Not Implemented
FC214 not included in watch window

# FC215 ENHANCED ANALOG SLAVE DEFINITION
FC215 block N+1 has state 0 GOOD
FC215 block N+1 has state 1 BAD
FC215 not included in watch window

# FC216 ENHANCED ANALOG INPUT DEFINITION
FC216 block N has quality
FC216 block N included in watch window

# FC217 ENHANCED CALIBRATION COMMAND
FC217 block N through N+4 included in watch window

# FC218 PHASEX Phase Execution
FC218 block N+3 has state 1 ABORT
FC218 block N+4 has state 0 AVAIL
FC218 block N+4 has state 1 AQUIRD
FC218 block N included in watch window

# FC219 COMMON SEQUENCE
FC219 block N through N+4 included in watch window

# FC220 BATCH HISTORIAN
FC220 block N has state 1 ALLBAD
FC220 block N+1 has state -1 NOTEXP
FC220 block N+1 has state 0  GOOD
FC220 block N+1 has state 1  BAD
FC220 block N+2 has state -1 NOTEXP
FC220 block N+2 has state 0  GOOD
FC220 block N+2 has state 1  BAD
FC220 block N+3 has state -1 NOTEXP
FC220 block N+3 has state 0  GOOD
FC220 block N+3 has state 1  BAD
FC220 block N+4 has state -1 NOTEXP
FC220 block N+4 has state 0  GOOD
FC220 block N+4 has state 1  BAD
FC220 block N+5 has state -1 NOTEXP
FC220 block N+5 has state 0  GOOD
FC220 block N+5 has state 1  BAD
FC220 block N+6 has state -1 NOTEXP
FC220 block N+6 has state 0  GOOD
FC220 block N+6 has state 1  BAD
FC220 block N+7 has state -1 NOTEXP
FC220 block N+7 has state 0  GOOD
FC220 block N+7 has state 1  BAD
FC220 block N+8 has state -1 NOTEXP
FC220 block N+8 has state 0  GOOD
FC220 block N+8 has state 1  BAD
FC220 block N through N+12 included in watch window

# FC221 IOD/DEV I/O Device Definition
FC221 block N-N+1 has quality
FC221 block N-N+1 has communication quality
FC221 block N has state 0 GOOD
FC221 block N has state 1 BAD
FC221 block N+1 has state 0 GOOD
FC221 block N+1 has state 1 BAD
FC221 block N+2 has state 1 OV-SIM
FC221 not included in watch window

# FC222 IOC/AIN Analog In/Channel
FC222 block N has quality
FC222 block N included in watch window

# FC223 IOC/AOUT Analog Out/Channel
FC223 block N has quality
FC223 block N included in watch window

# FC224 IOC/DIN Digital In/Channel
FC224 block N has quality
FC224 block N included in watch window

# FC225 IOC/DOUT Digital Out/Channel
FC225 block N has quality
FC225 block N included in watch window

# FC226 TEST STATUS Test Status
FC226 block N has state 0 FALSE
FC226 block N has state 1 TRUE
FC226 block N included in watch window

# FC227 Harmony Communication Block Configuration
FC227 block N-N+5 has quality
FC227 block N-N+5 has communication quality
FC227 block N has state 0 GOOD
FC227 block N has state 1 BAD
FC227 block N+1 has state 0 GOOD
FC227 block N+1 has state 1 BAD
FC227 block N+2 has state 0 GOOD
FC227 block N+2 has state 1 BAD
FC227 block N+3 has state 0 GOOD
FC227 block N+3 has state 1 BAD
FC227 block N+4 has state 0 GOOD
FC227 block N+4 has state 1 BAD
FC227 block N+5 has state 0 GOOD
FC227 block N+5 has state 1 BAD
FC227 not included in watch window

# FC228 Foreign Device Configuration
FC228 block N has quality
FC228 block N has state 0 GOOD
FC228 block N has state 1 BAD
FC228 not included in watch window

# FC229 Pulse In/Channel
FC229 block N has quality
FC229 block N included in watch window

# FC230 STRATEGIC LOOP CONTROLLER I/O
FC230 block N-N+13 has quality
FC230 block N+14 has state 0 GOOD
FC230 block N+14 has state 1 BAD
FC230 not included in watch window

# FC231 STRATEGIC LOOP CONTROLLER STATION
FC231 block N has state 1 ALARM
FC231 block N+1 has state 1 ACKNOW
FC231 block N+8 has state 0 MANUAL
FC231 block N+8 has state 1 AUTO
FC231 block N+9 has state 0 MANUAL
FC231 block N+9 has state 1 AUTO
FC231 block N+10 has state 0 MANUAL
FC231 block N+10 has state 1 AUTO
FC231 block N+11 has state 0 MANUAL
FC231 block N+11 has state 1 AUTO
FC231 block N+12 has state 1 BYPASS
FC231 block N+13 has state 1 LNKBAD
FC231 not included in watch window

# FC232 Not Implemented
FC232 not included in watch window

# FC233 Not Implemented
FC233 not included in watch window

# FC234 Not Implemented
FC234 not included in watch window

# FC235 Not Implemented
FC235 not included in watch window

# FC236 Not Implemented
FC236 not included in watch window

# FC237 Not Implemented
FC237 not included in watch window

# FC238 Not Implemented
FC238 not included in watch window

# FC239 Not Implemented
FC239 not included in watch window

# FC240 Not Implemented
FC240 not included in watch window

# FC241 DISTRIBUTED SOE SEM-MFP INTERFACE
FC241 block N has quality
FC241 block N has state 0 NO_LOG
FC241 block N has state 1 LOGGED
FC241 block N+1 has state 0 GOOD
FC241 block N+1 has state 1 BAD
FC241 not included in watch window

# FC242 DISTRIBUTED SOE DIGITAL EVENT INTERFACE
FC242 block N-N+15 has quality
FC242 block N+16 has state 0 GOOD
FC242 block N+16 has state 1 BAD
FC242 block N through N+15 included in watch window

# FC243 DISTRIBUTED SOE MASTER EXECUTIVE
FC243 not included in watch window

# FC244 DISTRIBUTED SOE MFP-SEM INTERFACE
FC244 not included in watch window

# FC245 DISTRIBUTED SOE SED-SEM INTERFACE
FC245 not included in watch window

# FC246 DISTRIBUTED SOE TRIGGER DEFINITION
FC246 not included in watch window

# FC247 Condition Monitoring Module
FC247 block N-N+11 has quality
FC247 block N+10 has state 0 OK
FC247 block N+10 has state 1 ALARM
FC247 block N+11 has state 0 OK
FC247 block N+11 has state 1 ALARM
FC247 block N+12 has state 0 GOOD
FC247 block N+12 has state 1 BAD
FC247 block N through N+9 included in watch window

# FC248 Not Implemented
FC248 block N-N+19 has quality
FC248 block N+4 through N+19 included in watch window

# FC249 Not Implemented
FC249 not included in watch window

# FC250 Not Implemented
FC250 not included in watch window

# FC251 Not Implemented
FC251 not included in watch window

# FC252 Not Implemented
FC252 not included in watch window

# FC253 Not Implemented
FC253 not included in watch window

# FC254 Not Implemented
FC254 not included in watch window

# FC255 BASIC BLOCK
FC255 not included in watch window

# CLIF FC20 CLIF PULSE TRIG
CLIF20 block N through N+1 included in watch window
CLIF20 S1 included in watch window

# CLIF FC21 CLIF C-SWITCH V-D
CLIF21 block N through N+8 included in watch window
CLIF21 S1 through S16 included in watch window

# CLIF FC22 CLIF C-SWITCH &-D
CLIF22 block N through N+8 included in watch window
CLIF22 S1 through S16 included in watch window

# CLIF FC23 CLIF C-SWITCH VS-D
CLIF23 block N through N+8 included in watch window
CLIF23 S1 through S16 included in watch window

# CLIF FC32 CLIF BOBIT
CLIF32 block N included in watch window

# CLIF FC47 CLIF WINDOW
CLIF47 block N through N+1 included in watch window
CLIF47 S1 through S3 included in watch window

# CLIF FC49 CLIF COMPAR
CLIF49 block N through N+2 included in watch window
CLIF49 S1 through S3 included in watch window

# CLIF FC61 CLIF SEQR STEP
CLIF61 block N through N+5 included in watch window
CLIF61 S1 through S39 included in watch window

# CLIF FC70 CLIF TIMER
CLIF70 block N through N+2 included in watch window
CLIF70 S1 through S3 included in watch window

# CLIF FC73 CLIF INTEGRATE
CLIF73 block N through N+8 included in watch window
CLIF73 S1 through S13 included in watch window

# CLIF FC87 CLIF SEQR BOOL OUT
CLIF87 block N through N+15 included in watch window
CLIF87 S1 through S18 included in watch window

# CLIF FC88 CLIF KEYBD DIG
CLIF88 block N included in watch window
CLIF88 S1 through S4 included in watch window

# CLIF FC100 CLIF KEYBD REAL
CLIF100 block N included in watch window
CLIF100 S1 through S6 included in watch window

# CLIF FC107 CLIF MINMAX
CLIF107 block N through N+1 included in watch window
CLIF107 S1 through S7 included in watch window

# CLIF FC131 CLIF SQRT
CLIF131 block N through N+1 included in watch window
CLIF131 S1 included in watch window

# CLIF FC158 CLIF C-SWITCH RX-A
CLIF158 block N through N+15 included in watch window
CLIF158 S1 through S16 included in watch window

# CLIF FC159 CLIF C-SWITCH RX-D
CLIF159 block N through N+15 included in watch window
CLIF159 S1 through S16 included in watch window

# CLIF FC176 CLIF LATCH
CLIF176 block N included in watch window
CLIF176 S1 through S2 included in watch window

# CLIF FC182 CLIF DIVIDE
CLIF182 block N through N+1 included in watch window
CLIF182 S1 through S2 included in watch window

# CLIF FC232 CLIF SWITCH HIGH
CLIF232 block N included in watch window
CLIF232 S1 through S3 included in watch window

# CLIF FC233 CLIF SWITCH LOW
CLIF233 block N included in watch window
CLIF233 S1 through S3 included in watch window

# CLIF FC234 CLIF RAMP
CLIF234 block N through N+1 included in watch window
CLIF234 S1 through S5 included in watch window

# CLIF FC235 CLIF ANALOG SELECTOR SWITCH
CLIF235 block N through N+1 included in watch window
CLIF235 S1 through S11 included in watch window

# CLIF FC236 CLIF DIGITAL SELECTOR SWITCH
CLIF236 block N through N+1 included in watch window
CLIF236 S1 through S11 included in watch window

# CLIF FC237 CLIF SWITCH X-ANALOG
CLIF237 block N through N+11 included in watch window
CLIF237 S1 through S8 included in watch window

# CLIF FC238 CLIF SWITCH X-DIGITAL
CLIF238 block N through N+9 included in watch window
CLIF238 S1 through S16 included in watch window

# CLIF FC239 CLIF DIGITAL INPUT SUBSTITUTION
CLIF239 block N-N+13 has quality
CLIF239 block N propagates quality from S1
CLIF239 block N+1 propagates quality from S2
CLIF239 block N+2 propagates quality from S3
CLIF239 block N+3 propagates quality from S4
CLIF239 block N+4 propagates quality from S5
CLIF239 block N+5 propagates quality from S6
CLIF239 block N+6 propagates quality from S7
CLIF239 block N+7 propagates quality from S8
CLIF239 block N+8 propagates quality from S9
CLIF239 block N+9 propagates quality from S10
CLIF239 block N+10 propagates quality from S11
CLIF239 block N+11 propagates quality from S12
CLIF239 block N+12 propagates quality from S13
CLIF239 block N+13 propagates quality from S14
CLIF239 block N through N+14 included in watch window
CLIF239 S1 through S14 included in watch window

# CLIF FC240 CLIF ANALOG INPUT SUBSTITUTION
CLIF240 block N-N+14 has quality
CLIF240 block N propagates quality from S1
CLIF240 block N+1 propagates quality from S2
CLIF240 block N+2 propagates quality from S3
CLIF240 block N+3 propagates quality from S4
CLIF240 block N+4 propagates quality from S5
CLIF240 block N+5 propagates quality from S6
CLIF240 block N+6 propagates quality from S7
CLIF240 block N+7 propagates quality from S8
CLIF240 block N+8 propagates quality from S9
CLIF240 block N+9 propagates quality from S10
CLIF240 block N+10 propagates quality from S11
CLIF240 block N+11 propagates quality from S12
CLIF240 block N+12 propagates quality from S13
CLIF240 block N+13 propagates quality from S14
CLIF240 block N+14 propagates quality from S15
CLIF240 block N through N+15 included in watch window
CLIF240 S1 through S15 included in watch window

# CLIF FC244 CLIF COUNT UP WITH HOLD
CLIF244 block N through N+2 included in watch window
CLIF244 S1 through S3 included in watch window

# CLIF FC245 CLIF COUNT DOWN
CLIF245 block N through N+2 included in watch window
CLIF245 S1 through S3 included in watch window

# CLIF FC246 CLIF LOOKUP TABLE
CLIF246 block N through N+1 included in watch window
CLIF246 S1 through S9 included in watch window
