Tag List

Client CQE
Client HGP - older, pre: 110 TAGTYPESRC  C 8 - WinCAD addition in 50017w.DBF     


Data file: td_571.DBF
Number of records: 0

Field   Name       Type   Width  Dec
  1     TAGINDEX    N        5     
  2     TAGNAME     C       14     
  3     TAGDESC     C       32     
  4     CUSTTAGID   C       32     
  5     TAGTYPE     C        7     
  6     EUDESC      C        6     
  7     EUINDEX     N        3     
  8     VAL0        N       11    1
  9     SPAN        N       11    1
 10     SETPTVAL0   N       11    1
 11     NUMDECPL    N        1     
 12     ZEROSTATE   C        6     
 13     ONESTATE    C        6     
 14     TWOSTATE    C        6     
 15     THREESTATE  C        6     
 16     FB1_0STATE  C        6     
 17     FB1_1STATE  C        6     
 18     FB2_0STATE  C        6     
 19     FB2_1STATE  C        6     
 20     FB3_0STATE  C        6     
 21     FB3_1STATE  C        6     
 22     FB4_0STATE  C        6     
 23     FB4_1STATE  C        6     
 24     LOOP        N        3     
 25     PCU         N        3     
 26     MODULE      N        2     
 27     BLOCK       N        4     
 28     ALMSTATE    C        6     
 29     ALARMTYPE   C        3     
 30     HALARM      N       11    1
 31     H2ALARM     N       11    1
 32     H3ALARM     N       11    1
 33     LALARM      N       11    1
 34     L2ALARM     N       11    1
 35     L3ALARM     N       11    1
 36     ALARMDB     N       11    1
 37     HVARALMTAG  N        5     
 38     H2DELTA     N       11    1
 39     H3DELTA     N       11    1
 40     LVARALMTAG  N        5     
 41     L2DELTA     N       11    1
 42     L3DELTA     N       11    1
 43     ALMINHTAG   N        5     
 44     ALMINHST    C        2     
 45     PRIMDISP    C        8     
 46     ALMGROUP    N        2     
 47     ALMACKBC    C        1     
 48     ALMACKNL    N        2     
 49     ALMACKTR    C        1     
 50     ALMSILTR    C        1     
 51     ADSKEYBD    N        2     
 52     ADSPANEL    N        2     
 53     ADSLAMP     N        2     
 54     PR_ALARM    C        1     
 55     SV_ALARM    C        1     
 56     PR_STCHNG   C        1     
 57     SV_STCHNG   C        1     
 58     PR_OPACT    C        1     
 59     SV_OPACT    C        1     
 60     MODTYPE     C        8     
 61     MODREV      C        2     
 62     APTASK      C        8     
 63     APSTATE     C        2     
 64     TP0TYPE     N        2     
 65     TP1TYPE     N        2     
 66     ARCHIVE     C        1     
 67     TP0LANG     N        1     
 68     TP1LANG     N        1     
 69     PM1_0STATE  C        6     
 70     PM1_1STATE  C        6     
 71     PM2_0STATE  C        6     
 72     PM2_1STATE  C        6     
 73     TEXT_SET    N        3     
 74     DEV_TYPE    C       16     
 75     DEV_NUMBER  N        1     
 76     DEVSUBTYPE  C       16     
 77     ALRM_PRTY1  N        1     
 78     ALRM_PRTY2  N        1     
 79     ALRM_PRTY3  N        1     
 80     ALRM_PRTY4  N        1     
 81     ALRM_PRTY5  N        1     
 82     ALRM_PRTY6  N        1     
 83     ALRM_PRTY7  N        1     
 84     ALRM_PRTY8  N        1     
 85     ALRM_PRTY9  N        1     
 86     ALRM_PRTYA  N        1     
 87     ALRM_PRTYB  N        1     
 88     ALRM_PRTYC  N        1     
 89     PID_BLOCK   N        4     
 90     SEC_LEVEL   N        2     
 91     SEC_GROUP   N        2     
 92     ALRMCMNT01  N        5     
 93     ALRMCMNT02  N        5     
 94     ALRMCMNT03  N        5     
 95     ALRMCMNT04  N        5     
 96     ALRMCMNT05  N        5     
 97     ALRMCMNT06  N        5     
 98     ALRMCMNT07  N        5     
 99     ALRMCMNT08  N        5     
100     ALRMCMNT09  N        5     
101     ALRMCMNT10  N        5     
102     ALRMCMNT11  N        5     
103     CNTRLENABL  C        1     
104     STR_LENGTH  N        2     
105     PRIMDSPCRT  N        2     
106     ALRM_PRTYD  N        1     
107     ALRM_PRTYE  N        1     
108     ALRMCMNT12  N        5     
109     ALRMCMNT13  N        5     
** Record Length **         571

Data file: cstags.TTG
  Record length: 570
  DBF Record length: 571
  Record count: 5396

